( TL19E00D52100000000FAAT05 )

VSA System Symptom Troubleshooting - ABS indicator, brake system indicator, VSA indicator, and TSA warning do not go off at the same time

1. Measure the voltage between VSA modulator-control unit 47P connector terminal No. 8 and body ground.

Is there battery voltage?

YES | - | Go to Step 15 .
NO | - | Repair open in the wire between the No. 6 (7.5 A) fuse in the driver's under-dash fuse/relay box and the VSA modulator-control unit.■

1. Turn the ignition switch to LOCK (0).