( TL19E00K791000R7312FAAT00 )

DTC Troubleshooting: 73-12

1. Check resistance between the No. 1 and No. 2 terminals of the left side E-pretensioner motor. There should be 0−1.0 Ω.

Is the resistance as specified?

YES | - | Open in the left engine compartment subharness (LHD models), the E-pretensioner subharness (RHD models), left side wire harness or left engine compartment wire harness; replace the faulty harness.■
NO | - | Faulty left side E-pretensioner motor; replace the left side E-pretensioner motor. ■