( TL19E00F00000057116KBAT00 )

Steering Gearbox Mount Cushion Replacement

1. Apply a mild soap and water solution to the new gearbox mount cushion surface (A), then place it on the gearbox mounting cushion hole.

1. Position the 36 mm socket wrench on the flange part of the gearbox housing with a washer, a flange bolt, and the nut as shown.

1. Install the gearbox mount cushion by tightening the flange bolt until the mount cushion edges (B) properly fit on the gearbox flange surface.

1. Install the steering gearbox.