( TL19E2AA20300024601CAAT00 )

ECM/PCM Inputs and Outputs at Connector A (□) (44P)
NOTE: Standard battery voltage is about 12 V.

Terminal number | Wire color | Terminal name | Description | Signal
--- | --- | --- | --- | ---
39 | ORN | BKSWNC (BRAKE PEDAL POSITION SWITCH) | Detects brake pedal position switch signal | With ignition switch ON (II) and brake pedal released: battery voltage With ignition switch ON (II) and brake pedal pressed: about 0 V
40 | LT GRN | BKSW (BRAKE PEDAL POSITION SWITCH) | Detects brake pedal position switch signal | With brake pedal released: about 0 V With brake pedal pressed: battery voltage
41 *2 | BRN | CRMTCLS (CRUISE CLUTCH PEDAL POSITION SIGNAL) | Detects clutch pedal position switch signal | With ignition switch ON (II) and clutch pedal released: about 0 V With ignition switch ON (II) and clutch pedal pressed: battery voltage
42 | RED | WEN (WRITE ENABLE SIGNAL) | Detects write enable signal | With ignition switch ON (II): about 0 V
43 *1 | PUR | SDNP (PADDLE SHIFTER− (DOWNSHIFT SWITCH)) | Detects (paddle shifter− (downshift switch)) signal | With paddle shifter− (downshift switch) pulled: about 0 V With paddle shifter− (downshift switch) released: about 5.0 V
43 *3 | RED/GRN | CLSW2 (CLUTCH SWITCH 2) | Detects clutch switch (SIL) signal | With ignition switch ON (II) and clutch pedal released: battery voltage With ignition switch ON (II) and clutch pedal pressed: about 0 V
44 | LT GRN | S-NET5V (SERIAL COMMUNICATION FOR IMMOBILIZER) | Sends serial communication signal | With ignition switch ON (II): pulses (about 4.4 V) With ignition switch OFF: about 1.4 V

*1: | A/T
*2: | M/T with cruise control
*3: | KE, KG, KR models (M/T)