( TL19E00G10110112011FEAT00 )

A/C Compressor Clutch Check

1. R20A3 engine model: Check for continuity between the A/C compressor clutch connector No. 1 and No. 3. If there is no continuity, replace the thermal protector.
   NOTE: The thermal protector will have no continuity above about 122 to 128 °C (252 to 262 °F). When the temperature drops below about 116 to 104 °C (241 to 219 °F), the thermal protector will have continuity.