( TL19E00B20200019101KDAT00 )

Front Damper/Spring Removal and Installation

1. Install the damper fork (A) over the driveshaft and onto the lower arm (B). Install the aligning tab (C) on the damper unit into the slot (D) of the damper fork.

1. Loosely install the damper pinch bolt (E) into the damper fork.

1. Connect the damper fork and the lower arm with the new damper fork mounting bolt (F), then lightly tighten the new mounting nut (G).

1. Place a floor jack under the lower arm, and raise the suspension to load it with the vehicle's weight.

1. Tighten the damper pinch bolt and the damper fork mounting nut while holding the mounting bolt to the specified torque values.

1. Tighten the damper mounting nuts and front strut brace mounting nuts on top of the damper to the specified torque values.