( TL19E00J54300065721KBAT00 )

Wiper Motor Replacement

1. Separate the linkage (A) from the link (B).

1. Note the positions (C), then remove the nut (D) and the link from the wiper motor (E).

1. Remove the three bolts, and separate the wiper motor from the linkage (F).

1. Before installing the motor, connect the 4P connector to the wiper motor, and turn the wiper/washer switch ON to (LO) or (HI) position, then OFF to return the motor shaft to the park position.
   NOTE:
   - Do not use the wiper/washer switch (INT) position in this step.
   - If necessary, replace any damaged clips.
   - Apply multipurpose grease to the moving parts.

1. Install the wiper motor to the wiper linkage assembly in the reverse order of removal.