( TL19E00K738000Y2476FAAT00 )

DTC Troubleshooting: B2476

1. Check for continuity between the headlight leveling control unit 16P connector No. 4 terminal and body ground.

Is there continuity?

YES | - | Replace the headlight leveling control unit .■
NO | - | Repair an open in the wire.■

1. Check the parameter of the front suspension stroke sensor with the HDS.

Is less than 0.4 V indicated?

YES | - | Go to Step 16 .
NO | - | Go to Step 23 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the front suspension stroke sensor 3P connector.

1. Disconnect the headlight leveling control unit 16P connector.