( TL19E00J26273455795KDAT00 )

Interior Trim Removal/Installation - Trunk Area

Rear Wheelhouse Insulator - For Some Models
NOTE: Put on gloves to protect your hands.

1. Remove the trunk side trim panel.

1. Detach the clips (A) and the harness holders (B) from the stud bolts, and detach the side wire harness clips (C), then remove the rear wheelhouse insulator (D).

1. Install the insulator in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips and the harness holders into place securely.