( TL19E00J18573560311KBAT00 )

Trunk Lid Latch Replacement

1. Install the latch in the reverse order of removal, and note these items:
   - Make sure the connector is plugged in properly and the opener cable is connected properly.
   - Make sure the trunk lid opens properly and locks securely.
   - Fix the original position of the outer end of cable (A) on the trunk lid latch securely. And check the trunk lid latch operation: Make sure the trunk lid latch unlock when turning the trunk lid cylinder with a key. If necessary, adjust the position of the cable end.