( TL19E20A14400049001NAAT00 )

Radiator

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Radiator | Coolant capacities (including engine, heater, hoses, and reservoir) Use genuine Honda All Season Antifreeze/Coolant Type 2 (LHD) | A/T: engine overhaul | 6.9 L (1.83 US gal, 1.52 Imp gal)
A/T: coolant change | 5.5 L (1.45 US gal, 1.21 Imp gal)
M/T: engine overhaul | 7.0 L (1.85 US gal, 1.54 Imp gal)
M/T: coolant change | 5.6 L (1.48 US gal, 1.23 Imp gal)
Coolant capacities (including engine, heater, hoses, and reservoir) Use genuine Honda All Season Antifreeze/Coolant Type 2 (RHD) | A/T: engine overhaul | 6.9 L (1.82 US gal, 1.52 Imp gal)
A/T: coolant change | 5.4 L (1.42 US gal, 1.18 Imp gal)
M/T: engine overhaul | 7.0 L (1.85 US gal, 1.54 Imp gal)
M/T: coolant change | 5.6 L (1.48 US gal, 1.23 Imp gal)