( TL19E00K791000R611XFAAT02 )

DTC Troubleshooting: 61-1x - Without Seat Heater

1. Measure the resistance between the No. 1 terminal of the SRS floor wire harness 2P connector and body ground. There should be 0−1.0 Ω.

Is resistance as specified?

YES | - | Faulty left side seat belt buckle switch; replace the left side seat belt buckle assembly. ■
NO | - | Open in the SRS floor wire harness; replace the SRS floor wire harness.■