( TL19E10K791000R111XFAAT00 )

DTC Troubleshooting: 11-1x

1. Install a jumper wire between the No. 2 and the No. 3 terminals of the dashboard wire harness 4P connector.

1. Do the battery terminal reconnection procedure.

1. Read the DTC.

Is DTC 11-1x indicated?

YES | - | Go to Step 16 .
NO | - | Open in the cable reel; replace the cable reel. ■

1. Turn the ignition switch to LOCK (0).

1. Do the battery terminal disconnection procedure , then wait for 3 minutes.

1. Disconnect SRS unit connector A (39P) from the SRS unit.