( TL19E20A18316200000MAAT00 )

Connecting Rod and Crankshaft End Play Inspection

1. Remove the oil pan.

1. Remove the balancer shaft/balancer shaft holder assembly.

1. Measure the connecting rod end play with a feeler gauge between the connecting rod and the crankshaft.

   Connecting Rod End Play
   Standard (New): | 0.15−0.35 mm (0.006−0.014 in.)
   Service Limit: | 0.45 mm (0.018 in.)

1. If the connecting rod end play is beyond the service limit, install a new connecting rod, and recheck. If it is still beyond the service limit; replace the crankshaft.