( TL19E1PE10411619621KBAT00 )

A/T Differential Carrier, Final Driven Gear Replacement

1. Remove the final driven gear (A) from the differential carrier (B).
   NOTE: Differential carrier bolts have left-hand threads.

1. Install the final driven gear in the direction shown on the differential carrier.

1. Secure the final drive gear and the differential carrier with the bolts. Tighten the bolts to the specified torque in a crisscross pattern in at least two steps.