( TL19E20A20326924001KBAT00 )

ELD Replacement

1. Do the battery terminal disconnection procedure.

1. Remove the upper cover (A), then remove the two positive (+) terminals (B).

1. Remove the under-hood fuse/relay box (C) from the bracket.

1. Remove the lower cover (A).

1. Disconnect the ELD 3P connector (B).

1. Remove the fuses (A) and (B).

1. Release the three lock tabs (A), and remove the ELD (B).

1. Install the parts in the reverse order of removal.

1. Do the battery terminal reconnection procedure.