( TL19E00J18535132001KBAT00 )

Hood Opener Cable Replacement

1. Disconnect the hood opener cable (A) from the hood release handle (B). Take care not to kink the cable.

1. Remove the grommet (C) from the body, then remove the hood opener cable from the vehicle. Take care not to kink the cable.

1. Install the cable in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - LHD model: When installing the opener cable under the dashboard, route the cable over the ground harness (D).
   - RHD model: When installing the opener cable under the dashboard, route the cable under the ground harness (E).

LHD model
RHD model