( TL19E00J34600000000CAAT00 )

Security Alarm System
The driver's MICU controls the turn signal lights and horns based upon the input signals of each switch and the B-CAN signals.

| Input | Output
--- | --- | ---

Driver's MICU

IG1 power supply
Ignition key switch
Driver's door switch
Left [right] rear door switch
Trunk lid latch switch
Left [right] rear door lock knob switch (UNLOCK)
Hood switch

Left turn signal lights
Right turn signal lights
Horns

B-CAN

Audio switch
Front passenger's door switch
Right [left] rear door switch
Driver's door key cylinder switch (LOCK/UNLOCK)
Driver's door lock knob switch (UNLOCK)
Front passenger's door lock switch (LOCK/UNLOCK)
Front passenger's door lock knob switch (UNLOCK)
Right [left] rear door lock knob switch (UNLOCK)
Keyless LOCK/UNLOCK signal

Driver's MICU (SET 1) signal
Driver's MICU (SET 2) signal
ALARM (ACTION) signal

[ ]: | RHD model