( TL19E00J18573560311KBAT00 )

Trunk Lid Latch Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the trunk lid.
- When removing components, use the trim tools or equivalent.

1. If equipped, remove the trunk lid trim panel.

1. From the latch cover (A) opening, pry the cover to release the projections (B) of the trunk lid latch (C) with the appropriate trim tool while pulling the cover, and release the projections (D) of the cover from the latch, then remove the cover.

1. Disconnect the trunk lid latch connector (E), and remove the bolts, then remove the trunk lid latch.