( TL19E00J34200057260KBAT00 )

Sunroof Drain Channel Slider and Cable Assembly Replacement

1. Install the slider and cable assembly in the reverse order of removal, and note these items:
   - Damaged parts should be replaced.
   - Apply multipurpose grease to the glass bracket (A) and the guide rail portion of the frame (B) indicated by the arrows.
   - Before reinstalling the motor, make sure both link lifters are parallel, and in the tilt-up position.
   - Before reinstalling the motor, install the frame and the glass, then check the opening drag.
   - After reinstalling the motor, reset the sunroof control unit.