( TL19E00K791000R7661FAAT00 )

DTC Troubleshooting: 76-61, 76-62

1. Check resistance between the No. 1 terminal of SRS unit connector B (39P) and body ground. There should be an open circuit or at least 1 MΩ.

Is the resistance as specified?

YES | - | Go to Step 18 .
NO | - | Short to ground between the No. 1 terminal of SRS unit connector B (39P) and the No. 6 terminal of the left engine compartment subharness 14P connector (LHD models) or E-pretensioner subharness 14P connector (RHD models).■