( TL19E3PK77100090986FAAT00 )

DTC Troubleshooting: P0986 (61)

DTC P0986:
Open in Shift Solenoid Valve E Circuit
NOTE:

- Before you troubleshoot, record all freeze data and any on-board snapshot with the HDS, and review General Troubleshooting Information.
- This code is caused by an electrical circuit problem and cannot be caused by a mechanical problem in the transmission.

K24Z3 Engine Model

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Start the engine with the shift lever in N, and wait for at least 1 second.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0986 indicated?

YES | - | Go to Step 8 .
NO | - | Go to Step 5 .

1. Select Shift Solenoid Valve E in the Miscellaneous Test Menu, and test shift solenoid valve E with the HDS.

Is a clicking sound heard?

YES | - | Go to Step 6 .
NO | - | Go to Step 8 .

1. Start the engine with the shift lever in N, and wait for at least 1 second.

1. Monitor the OBD STATUS for P0986 in the DTCs MENU with the HDS.

Does the HDS indicate FAILED?

YES | - | Go to Step 8 .
NO | - | If the HDS indicates PASSED, intermittent failure, the system is OK at this time. Check for poor connections or loose terminals between shift solenoid valve E and the PCM. If the HDS indicates NOT COMPLETED, go to Step 5 .

1. Turn the ignition switch to LOCK (0).

1. Jump the SCS line with the HDS.

1. Disconnect PCM connectors B (49P) and C (49P).

1. Measure the resistance between PCM connector terminals B25 and C44.

Is there 12−25 Ω?

YES | - | Go to Step 22 .
NO | - | Go to Step 12 .

1. Disconnect the shift solenoid wire harness connector.

1. Check for continuity between PCM connector terminal B25 and shift solenoid wire harness connector terminal No. 3.

Is there continuity?

YES | - | Go to Step 14 .
NO | - | Repair open in the wire between PCM connector terminal B25 and the shift solenoid wire harness connector, then go to Step 16 .

1. Remove the shift solenoid wire harness.

1. Check for continuity between shift solenoid wire harness connector terminal No. 3 and the shift solenoid valve E connector terminal.

Is there continuity?

YES | - | Replace shift solenoid valve E, then go to Step 16 .
NO | - | Replace the shift solenoid wire harness, then go to Step 16 .

1. Reconnect all connectors.

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Start the engine, with the shift lever in P, and wait for at least 1 second. Then shift to N, and wait for at least 1 second.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0986 indicated?

YES | - | Check for poor connections or loose terminals between shift solenoid valve E and the PCM, then go to Step 1 .
NO | - | Go to Step 21 .

1. Monitor the OBD STATUS for P0986 in the DTCs MENU with the HDS.

Does the HDS indicate PASSED?

YES | - | Troubleshooting is complete. If any other Temporary DTCs or DTCs were indicated in Step 20 , go to the indicated DTC's troubleshooting.■
NO | - | If the HDS indicates FAILED, check for poor connections or loose terminals between shift solenoid valve E and the PCM, then go to Step 1 . If the HDS indicates NOT COMPLETED, go to Step 19 .

1. Reconnect all connectors.

1. Update the PCM if it does not have the latest software, or substitute a known-good PCM.

1. Start the engine, with the shift lever in P, and wait for at least 1 second. Then shift to N, and wait for at least 1 second.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0986 indicated?

YES | - | Check for poor connections or loose terminals between shift solenoid valve E and the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 24 . If the PCM was substituted, go to Step 1 .
NO | - | Go to Step 26 .

1. Monitor the OBD STATUS for P0986 in the DTCs MENU with the HDS.

Does the HDS indicate PASSED?

YES | - | If the PCM was updated, troubleshooting is complete. If the PCM was substituted, replace the original PCM. If any other Temporary DTCs or DTCs were indicated in Step 25 , go to the indicated DTC's troubleshooting.■
NO | - | If the HDS indicates FAILED, check for poor connections or loose terminals between shift solenoid valve E and the PCM. If the PCM was updated, substitute a known-good PCM, then go to Step 24 . If the PCM was substituted, go to Step 1 . If the HDS indicates NOT COMPLETED, go to Step 24 .