( TL19E20A20336100000NAAT00 )

Engine idle

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Engine idle | Idle speed without load | M/T (in neutral) | 680±50 rpm (min −1 )
A/T (in N or P position) | 650±50 rpm (min −1 )
Idle speed with high electrical load (A/C switch ON, temperature set to max cool, blower fan on High, rear window defogger ON, and headlights on high beam) | M/T (in neutral), A/T (in N or P position) | 750±50 rpm (min −1 )
Idle CO |  | 0.1 % max.