( TL19E00K70900081610FAAT00 )

DTC Troubleshooting: 61

1. Check for continuity between the millimeter wave radar 5P connector No. 5 terminal and body ground.

Is there continuity?

YES | - | Repair a short to ground in the wire between the ACC unit and the millimeter wave radar.■
NO | - | Check for loose or poor connections. If the connections are OK, update the ACC unit, then recheck. If the ACC unit was already updated, replace the ACC unit. ■

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to ON (II).

1. Watch the ACC indicator and CMBS indicator.

Do the indicators come on?

YES | - | Go to Step 23 .
NO | - | Intermittent failure, the system is OK at this time.■

1. Check for DTCs with the HDS.

Is DTC 61 indicated?

YES | - | Check for loose or poor connections. If the connections are OK, replace the millimeter wave radar. After replacement, do the millimeter wave radar aiming. ■
NO | - | Troubleshoot the indicated DTC(s). If there are no DTCs, the system is OK at this time.■