( TL19E00J54300065001KBAT00 )

Washer Reservoir Replacement

1. Remove the front bamper.

1. Disconnect the 2P connector(s) (A) from the washer motor(s) (B).

   Washer Reservoir Capacity:
   4.5 L (4.8 US qt, 4.0 Imp qt): | KE, KG, KQ, KN (Without headlight washer) models
   5.0 L (5.3 US qt, 4.4 Imp qt): | KE, KG, KQ, KR (With headlight washer) models

1. Disconnect the washer tube(s) (C), then if necessary, remove the washer motor from the reservoir.
   NOTE: Fluid may flow out of the opening.