( TL19E00E16236500000LDAT00 )

Intermediate Shaft Reassembly

1. Install a new outer seal (A) into the bearing support (B) using the 45 mm installer attachment (C), 64 mm oil seal driver (D), the half shaft base (E), and a press.
   - R20A3 engine model: Press the seal until it is 0±0.2 mm (0±0.008 in.) below the surface of the bearing support end.
   - K24Z3 engine model: Press the seal until it is 4±0.2 mm (0.16±0.008 in.) below the surface of bearing support end.