( TL19E00B20200036401KBAT00 )

Front Knuckle/Hub/Wheel Bearing Replacement

1. Remove the cotter pin (A) from the upper arm ball joint, then remove the castle nut (B).
   NOTE: During installation, insert the new cotter pin into the ball joint pin hole from the front to the rear of the vehicle, and bend its end as shown. Check the ball joint pin hole direction before connecting the ball joint.

1. Disconnect the upper arm ball joint from the knuckle using the ball joint remover.