( TL19E00B44100017251KBAT00 )

Rear Control Arm Replacement

1. Raise the rear of the vehicle, and support it with safety stands in the proper locations.

1. Remove the rear wheel.

1. Remove the control arm mounting self-locking nut (A) and the washer (B) from the knuckle side.
   NOTE: Use a new self-locking nut during reassembly.

1. Mark the cam positions of the adjusting bolt (C) and the adjusting cam plate (D) with the frame.

1. Remove the self-locking nut (E) while holding the adjusting bolt, then remove the adjusting cam plate, the adjusting bolt, and the control arm (F).
   NOTE: Use a new adjusting bolt and a new self-locking nut during reassembly.

1. Install the control arm in the reverse order of removal, and note these items:
   - First install all the components, and lightly tighten the bolts and the nuts, then raise the suspension to load it with the vehicle's weight before fully tightening to the specified torque values.
   - Position the broadscale surface of the cam on the adjusting bolt and the adjusting cam plate facing down.
   - Align the cam positions of the adjusting bolt and the adjusting cam plate with the marked positions on the frame when tightening the self-locking nut.
   - Before installing the wheel, clean the mating surfaces on the brake disc or the brake disc/drum and the inside of the wheel.

1. Check the wheel alignment, and adjust it if necessary.