( TL19E20A14674317531KDAT00 )

Crankshaft Pulley Removal and Installation

Special Tools Required
Handle, 6-25-660L
07JAB-001020B
Crankshaft pulley holder, 50 offset 65
070AB-RJA0100
Socket wrench, 19 x 90L
07JAA-001020A
Removal

1. Remove the right front wheel.

1. Remove the splash shield.

1. Remove the drive belt.

1. Hold the pulley with the handle (A) and the crankshaft pulley holder (B).

1. Remove the bolt with a 19 x 90L socket (C) and a breaker bar, then remove the crankshaft pulley.