( TL19E00J18573465521KBAT00 )

Windshield Side Trim Replacement

Trim Replacement
NOTE:

- Put on gloves to protect your hands.
- Take care not to damage the windshield.
- Do not use any metal tools to remove the windshield side trim, or you may chip the edge of the windshield and some cracks in the windshield will result.
- When removing components, use the trim tools or equivalent.
- Take care not to bend the windshield side trim.

1. Remove the windshield side trim (A).

   -1. | While pushing the upper retainer (B) portion of the trim to the pillar side by hand, gently pry up the trim to release the trim from the retainers.
   -2. | Gradually work your way down to release each of the retainers (C).
   -3. | Slide the trim rearward to release it from the bottom clip (D).