( TL19E00H46400055408KBAT00 )

Side Curtain Airbag Replacement

Removal
NOTE:

- Review the interior trim replacement procedure before doing repair or service.
- Removal of the side curtain airbag must be done according to Precaution and Procedures.
- The side curtain airbag system consists of many components. When the side curtain airbag has been deployed, go to Component Replacement/Inspection After Deployment, and replace all of the parts listed.

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Remove the headliner.

1. Disconnect the SRS floor wire harness 2P connectors (A) from the side curtain airbags.