( TL19E00H10800040231MBAT00 )

Millimeter Wave Radar Aiming

Horizontal Aiming

1. Park the vehicle to an open area with at least this much space in front of it: 10 m (32.8 ft) of distance, 4 m (13.1 ft) wide, and 1.2 m (3.9 ft) height.

1. Turn the ignition switch to LOCK (0).

1. Connect the HDS to the data link connector (A).

1. Turn the ignition switch to ON (II).

1. Check for DTCs with the HDS.
   NOTE: If DTC 61 or DTC 62 is indicated, troubleshoot the indicated DTC first.

1. Start the engine.