( TL19E00J4616185367BKBAT00 )

Front Seat Slide Motor Replacement

SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
8-way Power Seat
NOTE:

- Put on gloves to protect your hands.
- The driver's seat on LHD model is shown; the passenger's seat is symmetrical; the ones on RHD model are similar.

1. Remove the front seat.

1. Remove the seat cushion cover/pad.

1. Remove the flex cable (A) and the cable housing (B).

   -1. | Release the housing from the hooks (C).
   -2. | Disconnect the cable from the worm gear (D) in the inner seat track by pulling out the housing.
   -3. | Disconnect the cable from the slide motor (E). NOTE: Take care not to kink the cable.