( TL19E00J16126721401KDAT00 )

Front Door Panel Removal/Installation

1. Disconnect the inner handle cable (A) and the latch cable (B) from the inner handle (C), then remove the handle.

   -1. | Detach the inner handle cable fasteners (D, E), then disconnect the inner handle cable from the cable fasteners.
   -2. | Detach the latch cable fastener (F), and remove the latch cable fastener (G) from the inner handle by pinching its tabs out. NOTE: Check if the cable fasteners are damaged or stress-whitened.