( TL19E00J34600000000CAAT00 )

Headlight Washer Operation
The passenger's MICU controls the headlight washer motor based upon the input signals from the headlight washer switch, headlight switch and wiper switch.

| Input | Output
--- | --- | ---
Passenger's MICU | IG1 power supply Headlight washer switch | Headlight washer motor relay
B-CAN | Wiper switch signal Lighting switch signals (headlight low beam, headlight high beam) |