( TL19E00K722000R3207FAAT00 )

DTC Troubleshooting: 32-07

DTC 32-07:
EPS Control Unit Internal Circuit (Current Sensor) (Steering Diagnosis)

1. Turn the ignition switch to ON (II).

1. Clear the DTC with the HDS.

1. Turn the ignition switch to LOCK (0).

1. Start the engine.

1. Turn the steering wheel to the right or left, and wait 10 seconds or more.

1. Check for DTCs with the HDS.

Is DTC 32-07 indicated?

YES | - | Replace the EPS control unit. ■
NO | - | Intermittent failure, the system is OK at this time.■