( TL19E00J26220219251KDAT10 )

Dashboard Side Vent Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- The driver's side vent on the LHD model is shown; the passenger's side vent on the LHD model is symmetrical; the dashboard side vents on the RHD model are similar.

1. Driver's side: Open the front door, and remove the driver's dashboard side lid (A).

   -1. | Pull the lower edge of the lid by hand to detach the lower clip (B).
   -2. | Gently pull the rear edge of the lid outward by hand to detach the clips (C) and the hooks (D).
   -3. | Release the hooks (E, F).

1. Passenger's side: Open the glove box, then remove the passenger's dashboard side lid.