( TL19E00J26220257121KDAT00 )

Dashboard/Steering Hanger Beam Removal/Installation

1. Remove the special bolts (A) from outside the passenger's door. LHD model is shown; RHD model is symmetrical.

   -1. | Remove the caps (B).
   -2. | Loosen the special bolt until its threads have come off the side bracket (C) of the steering hanger beam. The bolt will be screwed into the inside threads of the collar bolt (D) by loosening the bolt. Because of the thread lock on the threads of the bolt, the bolt and the collar bolt will be fixed.
   -3. | Loosen the bolt again to screw the collar bolt into the fixed space adjuster (E) until it is stopped by the stopper (F). This will provide a gap (G) between the collar bolt and the body.
   -4. | Remove the bolts.