( TL19E00J16126720801KBAT00 )

Front Door Latch Replacement

Without Super Locking
NOTE: Put on gloves to protect your hands.

1. Remove these items:
   - Tweeter cover
   - Door panel
   - Inner handle
   - Door end trim

1. Raise the glass fully.

1. Remove the plastic cover as needed.

1. Detach the rod fastener, and disconnect the outer handle rod from the outer handle base.

1. Driver's door: Disconnect the cylinder cable from the latch.

1. Pull the glass run channel (A) away as needed, and remove the bolt, then remove the center lower channel (B) by pulling it downward.