( TL19E00J26200031201KDAT00 )

Headliner Removal/Installation

1. Remove the headliner (A) from the vehicle. LHD model is shown; RHD model is symmetrical.

   -1. | Lower the headliner.
   -2. | Move the headliner rearward.
   -3. | Lower the front of the headliner below the steering wheel.
   -4. | Rotate the headliner so as to point the front end to the outside of the passenger's front door and the rear end to the outside of the driver's front door.
   -5. | Pull the headliner along with the interior wire harness (B) and the antenna lead (C) out through the passenger's front door. NOTE: Do not bend the headliner. Bending the headliner will crease and damage it.