( TL19E20A18300043401KCAT00 )

Engine Oil Pan Installation

1. A/T model: Install the sift cable cover.

1. Install the intermediate shaft.

1. Install a new set ring on the end of right side driveshaft, then install the driveshaft. Make sure ring ‘‘clicks'' into place in the intermediate shaft.

1. Connect the right side knuckle to the lower arms.

1. Install exhaust pipe A. Use new gaskets and new self-locking nuts.

1. Install the A/C compressor.

1. Install the drive belt.

1. Refill the engine with engine oil.

1. Install the splash shield.