( TL19E00H46200053402KBAT00 )

Rear Seat Belt Replacement

1. Install the seat belt and buckles in the reverse order of removal, and note these items:
   - With rear seat belt switch: Make sure the seat belt switch connectors are plugged in properly.
   - Apply medium strength liquid thread lock to the center anchor bolts before reinstallation.
   - Tighten the bolts by hand first, then tighten to the specified torque.
   - Check that the retractor locking mechanism functions.
   - Assemble the washer on the center anchor bolt as shown.
   - Before installing the center anchor bolt, make sure there are no twists or kinks in the center seat belt.
   - Make sure the rear center ELR (emergency locking retractor) is pointing straight forward.

Center anchor bolt installation