( TL19E00J2621651641AKDAT00 )

Center Console Rear Trim Removal/Installation

NOTE:

- Take care not to scratch the center console and the related parts.
- When removing components, use the trim tools or equivalent.

1. Gently pull out the console rear trim (A) to detach the clips and to release both upper tabs (B) on the center console, then remove the trim. Rear ventilation type is shown; no rear ventilation type is similar.

1. With rear ventilation: Remove the screws, release the tabs (A), then remove the rear vent (B) from the rear trim (C).

1. Install the trim in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.