( TL19E00J18573417471KBAT00 )

Cowl Cover Replacement

NOTE:

- Put on gloves to protect your hands.
- When removing components, use the trim tools or equivalent.
- Take care not to damage the body.
- LHD model is shown; RHD model is symmetrical, except the tubing of the washer tube.

1. Remove these items:
   - Windshield wiper arms
   - Front grille cover
   - Front fender trim, both sides for some models

1. Remove the cowl cover (A).

   -1. | Remove the clips (B).
   -2. | Disconnect the washer tube (C).
   -3. | Detach the clips (D, E, F) by carefully pulling the cover up.
   -4. | Release two front hooks (G) from the body.
   -5. | Release the hood hinge covers (H) from both hood hinges (I).

1. Install the covers in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.
   - Make sure the hood hinge covers are seated on the cowl cover securely.
   - Make sure the washer tube is connected properly.