( TL19E00K791000R7661FAAT00 )

DTC Troubleshooting: 76-61, 76-62

1. Check resistance between the No. 2 terminals of the left engine compartment subharness 5P connector (LHD models) or E-pretensioner subharness 5P connector (RHD models) and body ground. There should be 0−1.0 Ω.

Are the resistances as specified?

YES | - | Go to Step 15 .
NO | - | Open between the No. 5 terminal of the left engine compartment subharness 5P connector (LHD models) or E-pretensioner subharness 5P connector (RHD models) and body ground or poor connection G303 (LHD models) or G251 (RHD models). ■

1. Do the battery terminal disconnection procedure, then wait for 3 minutes.

1. Disconnect SRS unit connector B (39P) form the SRS unit.