( TL19E00K791000R764XFAAT00 )

DTC Troubleshooting: 76-4x, 76-5x, 76-63

DTC 76-4x (‘‘x'' can be 0 thru 6, 9 or A thru F), 76-5x (‘‘x'' can be 0 thru 9 or A thru F), 76-63:
Internal Failure of E-pretensioner Unit

1. Clear the DTC memory.

1. Turn the ignition switch to ON (II), and check that the SRS indicator comes on for about 6 seconds and then goes off.

Does the SRS indicator stay on?

YES | - | Intermittent failure, the system is OK at this time. Go to Troubleshooting Intermittent Failures. If another DTC is indicated, troubleshoot the DTC.
NO | - | Replace the E-pretensioner unit. ■