( TL19E1PE10411619601KBAT00 )

A/T Differential Carrier Bearing Outer Race Replacement

Special Tools Required
Driver handle 15 x 135L
07749-0010000
Bearing driver attachment 78 x 80 mm
07NAD-PX40100
Bearing driver attachment 72 x 75 mm
07746-0010600
NOTE:

- The bearing and the bearing outer race should be replaced as a set.
- Replace the bearing with a new one whenever the outer race is replaced.
- Do not use the thrust shim from the torque converter housing.
- Adjust bearing preload after replacing the bearing and outer race.
- Cost all parts with ATF during installation.

1. Remove the bearing outer race (A), the 76.2 mm thrust washer (B), and the 76 mm thrust shim (C) from the transmission housing (D) by heating the transmission housing to about 100 °C (212 °F) using a heat gun (E). Do not heat the transmission housing more than 100 °C (212 °F).
   NOTE: Let the transmission housing cool to room temperature before installing the bearing outer race.