( TL19E20A14400059301KBAT00 )

Thermostat Replacement

1. Drain the engine coolant.

1. Remove the harness clamp bracket and the thermostat cover, then remove the thermostat.

1. Install the thermostat with a new rubber seal.

1. Refill the radiator with engine coolant, then bleed the air from the cooling system.

1. Clean up any spilled engine coolant.

1. Drain the engine coolant.

1. Remove the harness clamp bracket and the thermostat cover, then remove the thermostat.

1. Install the thermostat with a new rubber seal.

1. Refill the radiator with engine coolant, then bleed the air from the cooling system.

1. Clean up any spilled engine coolant.