( TL19E10K791000R118XFAAT00 )

DTC Troubleshooting: 11-8x

1. Measure the voltage between the No. 3 and the No. 4 terminals of SRS unit connector A (39P) and body ground. There should be less than 0.5 V.

Is the voltage as specified?

YES | - | Faulty driver's airbag; replace the driver's airbag. ■
NO | - | Go to Step 17 .

1. Turn the ignition switch to LOCK (0).

1. Do the battery terminal disconnection procedure , then wait for 3 minutes.