( TL19E00J54200034401KBAT00 )

Ignition Switch Replacement

SRS components are located in this area. Review the SRS component locations and precautions and procedures before performing repairs or servicing.

1. Do the battery terminal disconnection procedure.

1. Remove the steering column covers.

1. Disconnect the 5P connector (A) from the ignition switch (B).

1. Remove the two screws and the ignition switch.

1. Install the parts in the reverse order of removal.

1. Do the battery terminal reconnection procedure.